----------------------------------------------
Midland Railway steam engine 890 Class
Version 2.0 of September 2025
----------------------------------------------

62 Class 890 engines were built around 1872-74, in 1907 they were renumered.
Kirtley wanted those engines and Johnson rebuilt them in 1880-89.
They were fitted with the P boiler and screw reversing gear.


LMS Power classification: 1P
Configuration: 2-4-0 (120 - 1Bn2)
Boiler: P type at 140 psi , saturated steam
Tractive effort: 9660lb 
Max speed: not indicated
Cylinders: 2 inside
Diameter x stroke: 18x24in (457.7mm x 609.6mm) 
Diameter of driving wheels: 6ft 8&1/2in (2.045m)
Construction period: 1872-74


Pack content:

Steam Engine N°93 for express trains              setting from 1907 to 1923
Steam Engine N°121 for local trains               setting from 1907 to 1923



Installation:
1. Unzip all in main Train Simulator folder, checking if Winzip has checked
"Use folder    names" box.
2. Use the editor to make a consist.



- Repainter notice: this model can be freely repainted, but the repainted version
MUST give credit to the authors of this work, it can not be sold, and the author of
the repaint must tell me of his work and of a site to download it.

- This model is freeware.
This means it can be redistributed, but only if not modified: no files can be deleted
from this archive, and no files can be added to the archive without the author
authorization. This file can not be sold on the internet, or via optical or magnetic
storage devices, or in any other way: you can't make money from this file. The author
can ask sites publishing this file, to remove it. "Theft" of this material
(all the files in this archive) will not be tolerated.

Model and textures: Renzo Grassi, grassirenzo@yahoo.it
File ENG: Massimo Bruni, massimo.bruni76@gmail.com

